A map of a city

Description automatically generated

Methods: Soil samples were air dried, ground and screened through a 230 micron sieve. A recently calibrated XRF analyzer was used to measure the abundance of lead as well as other elements. Machine blanks were used to check for measurement drift.